# Changelog

All notable changes to this project will be documented in this file.

## [2.5] - 2025-06-05

### Fixed

- LE-01MWv2 LCD parameters error

## [2.4] - 2025-05-12

### Added

- support for LE-03Mv2 meter

## [2.3] - 2025-03-16

### Changed

- LE-01MWv2 LCD display bit pattern to reflect actual device

## [2.2] - 2023-12-19

### Fixed

- LE03MP "can't read 'top'" errors

## [2.1] - 2023-12-07

### Added

- support for LE-01DC meter

## [2.0] - 2023-11-17

### Changed

- tab view to droplist view
- find meter procedure split to 'find meter' and 'connect to meter'

### Fixed

- LE-03MQCTv2 meter search error due to new meter firmware

## [1.22] - 2023-10-02

### Fixed

- LE-03MQv2 meter search error due to new meter firmware

## [1.21] - 2023-07-27

### Fixed

- LE-03M and LE-03MCT find meter bug

## [1.20] - 2023-07-12

### Added

- new LE-01MWv2 meter support
- manual 'find meter' mode to connect meters with known parameters

### Fixed

- fix LE-03MQxx 'Pulse constant' set value

## [1.19] - 2023-05-30

### Fixed

- Fixed "invalid octal number" error for all tariff writings

## Old fashioned previous reversed changelog

### 1.4
-  Fixed reading error in LE Config for LE-03M-CT meter and CT value 125
### 1.5
-  Added LE-01MR, LE-03MW
### 1.6
-  Added LE-03MWCT, Fixed COMx read error for x > 9
### 1.7
-  Corrected for LE-03MCT transformation ratio 125:5
### 1.8
-  Added LE-01MW
### 1.9
-  Fixed for LE-01MW "frame format"
### 1.10
-  Fixed time for LE-01MW, LE-03MW, LE-03MWCT
### 1.11
-  Improved work with LE-03MWCT
### 1.12
-  Improved work with LE-03MWCT (Pulse Output Constant)
### 1.13
-  Fixed time reading error with LE-0xMWx
### 1.14
-  Added batch address configurations
### 1.15
-  Added for LE-03MWCT transformation ratios 30:5, 80:5, 750:5
### 1.16
-  Added LE-01MRv2, LE-01MWv2 (LE-01MWv2 temporary disabled)
### 1.17
-  Improved work with LE-01MQ
-  Energy display bug of LE-01MW and LE-01MR has been fixed
### 1.18
-  Added reading all energies for LE-01MW, LE-03MW, LE-03MWCT


